# **Vendor FRTC Questionnaire**

1. What smart card readers does the solution support for enrollment/registration?
2. What biometric readers does the solution support for enrollment/registration?
3. Does the product use Microsoft Windows CAPI or something else?
4. Does it use the ***Local Machine*** Certificate Store or the ***Current User*** Certificate Store if it uses Microsoft CAPI?
5. If Microsoft CAPI is not used, where do you install certificates for use in the product for FRTC?
6. Where are the OIDs registered/changed within the product?
7. Where are the logs that show the registration outcome?
8. Where are the logs that show the time of access outcome?
9. How do you disable certificate validation for registration?
10. How do you disable certificate validation for the time of access?
11. Does your solution rely on a validation process within the PACS software to change the user status for the time of access test cases to respond as expected?
12. What is the process for verifying the equipment table, specifically SW and FW versions?
13. How do you change authentication modes on the reader(s) (PKI-CAK, PKI-AUTH, PKI-CAK+BIO, PKI-AUTH+BIO)?
14. How can the negotiated bit rate on the contact reader be changed to 446 KBps? *(FRTC Test Case 5.18.01)*
15. How can the negotiated bit rate on the contactless reader be changed to 848 KBps? *(FRTC Test Case 5.18.02)*
16. How do you configure the software application to support using 128-bit FASC-N for Time of Registration and Time of Access?
17. How do you configure the software application to support using 128-bit UUID for Time of Registration and Time of Access?
18. Does the solution support the multifactor dynamic assignment of an individual reader authentication mode on a time-based schedule? *(FRTC Test Cases 7.07.05 & 7.07.06)* If yes, how is it configured?
19. The vendor shall provide a test data report documenting conformance for review and approval of contact readers shall support ISO/IEC 7816 *(FRTC Test Case 7.07.09)*
20. The vendor shall provide a test data report documenting conformance for review, and approval of contactless readers shall support ISO/IEC 14443 Type A *(FRTC Test Case 7.07.10)*
21. How do I determine what the PACS system uses as the primary identifier?
22. Does the solution leverage a cached copy of the public key extracted at the time of registration for signature verification at the Time of Access? (5.02.06)
23. Does the solution support SM-Auth?
24. Does the solution support OCC-Auth?
25. How do you turn on fingerprint verification required for enrollment/registration?
26. How do you turn off fingerprint verification required for enrollment/registration?
27. What objects/values are read from the PIV Card at enrollment?